{
  "schema": "xilinx.com:schema:json_instance:1.0",
  "ip_inst": {
    "xci_name": "NewExtInst_TOP_processing_system7_0_0",
    "cell_name": "processing_system7_0",
    "component_reference": "xilinx.com:ip:processing_system7:5.5",
    "ip_revision": "6",
    "gen_directory": "../../../../../../NewExtInst_Debug.gen/sources_1/bd/NewExtInst_TOP/ip/NewExtInst_TOP_processing_system7_0_0",
    "parameters": {
      "component_parameters": {
        "PCW_DDR_RAM_BASEADDR": [ { "value": "0x00100000", "value_src": "user", "resolve_type": "user", "format": "bitString", "usage": "all" } ],
        "PCW_DDR_RAM_HIGHADDR": [ { "value": "0x3FFFFFFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "usage": "all" } ],
        "PCW_UART0_BASEADDR": [ { "value": "0xE0000000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_UART0_HIGHADDR": [ { "value": "0xE0000FFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_UART1_BASEADDR": [ { "value": "0xE0001000", "value_src": "user", "resolve_type": "user", "format": "bitString", "usage": "all" } ],
        "PCW_UART1_HIGHADDR": [ { "value": "0xE0001FFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "usage": "all" } ],
        "PCW_I2C0_BASEADDR": [ { "value": "0xE0004000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_I2C0_HIGHADDR": [ { "value": "0xE0004FFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_I2C1_BASEADDR": [ { "value": "0xE0005000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_I2C1_HIGHADDR": [ { "value": "0xE0005FFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_SPI0_BASEADDR": [ { "value": "0xE0006000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_SPI0_HIGHADDR": [ { "value": "0xE0006FFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_SPI1_BASEADDR": [ { "value": "0xE0007000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_SPI1_HIGHADDR": [ { "value": "0xE0007FFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_CAN0_BASEADDR": [ { "value": "0xE0008000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_CAN0_HIGHADDR": [ { "value": "0xE0008FFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_CAN1_BASEADDR": [ { "value": "0xE0009000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_CAN1_HIGHADDR": [ { "value": "0xE0009FFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_GPIO_BASEADDR": [ { "value": "0xE000A000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_GPIO_HIGHADDR": [ { "value": "0xE000AFFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_ENET0_BASEADDR": [ { "value": "0xE000B000", "value_src": "user", "resolve_type": "user", "format": "bitString", "usage": "all" } ],
        "PCW_ENET0_HIGHADDR": [ { "value": "0xE000BFFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "usage": "all" } ],
        "PCW_ENET1_BASEADDR": [ { "value": "0xE000C000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_ENET1_HIGHADDR": [ { "value": "0xE000CFFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_SDIO0_BASEADDR": [ { "value": "0xE0100000", "value_src": "user", "resolve_type": "user", "format": "bitString", "usage": "all" } ],
        "PCW_SDIO0_HIGHADDR": [ { "value": "0xE0100FFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "usage": "all" } ],
        "PCW_SDIO1_BASEADDR": [ { "value": "0xE0101000", "value_src": "user", "resolve_type": "user", "format": "bitString", "usage": "all" } ],
        "PCW_SDIO1_HIGHADDR": [ { "value": "0xE0101FFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "usage": "all" } ],
        "PCW_USB0_BASEADDR": [ { "value": "0xE0102000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_USB0_HIGHADDR": [ { "value": "0xE0102fff", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_USB1_BASEADDR": [ { "value": "0xE0103000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_USB1_HIGHADDR": [ { "value": "0xE0103fff", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_TTC0_BASEADDR": [ { "value": "0xE0104000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_TTC0_HIGHADDR": [ { "value": "0xE0104fff", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_TTC1_BASEADDR": [ { "value": "0xE0105000", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_TTC1_HIGHADDR": [ { "value": "0xE0105fff", "value_src": "user", "resolve_type": "user", "format": "bitString", "enabled": false, "usage": "all" } ],
        "PCW_FCLK_CLK0_BUF": [ { "value": "TRUE", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_FCLK_CLK1_BUF": [ { "value": "TRUE", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_FCLK_CLK2_BUF": [ { "value": "TRUE", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_FCLK_CLK3_BUF": [ { "value": "TRUE", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_FREQ_MHZ": [ { "value": "533.333333", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_BANK_ADDR_COUNT": [ { "value": "3", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_ROW_ADDR_COUNT": [ { "value": "15", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_COL_ADDR_COUNT": [ { "value": "10", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_CL": [ { "value": "7", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_CWL": [ { "value": "6", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_T_RCD": [ { "value": "7", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_T_RP": [ { "value": "7", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_T_RC": [ { "value": "48.91", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_T_RAS_MIN": [ { "value": "35.0", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_T_FAW": [ { "value": "40.0", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_AL": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_TO_CLK_DELAY_0": [ { "value": "0.0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_TO_CLK_DELAY_1": [ { "value": "0.0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_TO_CLK_DELAY_2": [ { "value": "0.0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_TO_CLK_DELAY_3": [ { "value": "0.0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_BOARD_DELAY0": [ { "value": "0.25", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_BOARD_DELAY1": [ { "value": "0.25", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_BOARD_DELAY2": [ { "value": "0.25", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_BOARD_DELAY3": [ { "value": "0.25", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_0_LENGTH_MM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_1_LENGTH_MM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_2_LENGTH_MM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_3_LENGTH_MM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQ_0_LENGTH_MM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQ_1_LENGTH_MM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQ_2_LENGTH_MM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQ_3_LENGTH_MM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_0_LENGTH_MM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_1_LENGTH_MM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_2_LENGTH_MM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_3_LENGTH_MM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_0_PACKAGE_LENGTH": [ { "value": "76.687", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_1_PACKAGE_LENGTH": [ { "value": "77.8025", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_2_PACKAGE_LENGTH": [ { "value": "72.8405", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_3_PACKAGE_LENGTH": [ { "value": "111.904", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQ_0_PACKAGE_LENGTH": [ { "value": "73.119", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQ_1_PACKAGE_LENGTH": [ { "value": "63.8935", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQ_2_PACKAGE_LENGTH": [ { "value": "77.045", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQ_3_PACKAGE_LENGTH": [ { "value": "111.903", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_0_PACKAGE_LENGTH": [ { "value": "76.428", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_1_PACKAGE_LENGTH": [ { "value": "76.428", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_2_PACKAGE_LENGTH": [ { "value": "76.428", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_3_PACKAGE_LENGTH": [ { "value": "76.428", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_0_PROPOGATION_DELAY": [ { "value": "160", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_1_PROPOGATION_DELAY": [ { "value": "160", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_2_PROPOGATION_DELAY": [ { "value": "160", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQS_3_PROPOGATION_DELAY": [ { "value": "160", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQ_0_PROPOGATION_DELAY": [ { "value": "160", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQ_1_PROPOGATION_DELAY": [ { "value": "160", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQ_2_PROPOGATION_DELAY": [ { "value": "160", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DQ_3_PROPOGATION_DELAY": [ { "value": "160", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_0_PROPOGATION_DELAY": [ { "value": "160", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_1_PROPOGATION_DELAY": [ { "value": "160", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_2_PROPOGATION_DELAY": [ { "value": "160", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_3_PROPOGATION_DELAY": [ { "value": "160", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_PACKAGE_DDR_DQS_TO_CLK_DELAY_0": [ { "value": "-0.000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_PACKAGE_DDR_DQS_TO_CLK_DELAY_1": [ { "value": "-0.001", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_PACKAGE_DDR_DQS_TO_CLK_DELAY_2": [ { "value": "0.004", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_PACKAGE_DDR_DQS_TO_CLK_DELAY_3": [ { "value": "-0.035", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_PACKAGE_DDR_BOARD_DELAY0": [ { "value": "0.075", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_PACKAGE_DDR_BOARD_DELAY1": [ { "value": "0.070", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_PACKAGE_DDR_BOARD_DELAY2": [ { "value": "0.077", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_PACKAGE_DDR_BOARD_DELAY3": [ { "value": "0.094", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_CPU_CPU_6X4X_MAX_RANGE": [ { "value": "800", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_CRYSTAL_PERIPHERAL_FREQMHZ": [ { "value": "33.333333", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_APU_PERIPHERAL_FREQMHZ": [ { "value": "666.666666", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_DCI_PERIPHERAL_FREQMHZ": [ { "value": "10.159", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_QSPI_PERIPHERAL_FREQMHZ": [ { "value": "150", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_SMC_PERIPHERAL_FREQMHZ": [ { "value": "100", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_USB0_PERIPHERAL_FREQMHZ": [ { "value": "60", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_USB1_PERIPHERAL_FREQMHZ": [ { "value": "60", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_SDIO_PERIPHERAL_FREQMHZ": [ { "value": "100", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UART_PERIPHERAL_FREQMHZ": [ { "value": "100", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_SPI_PERIPHERAL_FREQMHZ": [ { "value": "166.666666", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_CAN_PERIPHERAL_FREQMHZ": [ { "value": "100", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_CAN0_PERIPHERAL_FREQMHZ": [ { "value": "-1", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_CAN1_PERIPHERAL_FREQMHZ": [ { "value": "-1", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_I2C_PERIPHERAL_FREQMHZ": [ { "value": "25", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_WDT_PERIPHERAL_FREQMHZ": [ { "value": "133.333333", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_TTC_PERIPHERAL_FREQMHZ": [ { "value": "50", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_TTC0_CLK0_PERIPHERAL_FREQMHZ": [ { "value": "133.333333", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_TTC0_CLK1_PERIPHERAL_FREQMHZ": [ { "value": "133.333333", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_TTC0_CLK2_PERIPHERAL_FREQMHZ": [ { "value": "133.333333", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_TTC1_CLK0_PERIPHERAL_FREQMHZ": [ { "value": "133.333333", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_TTC1_CLK1_PERIPHERAL_FREQMHZ": [ { "value": "133.333333", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_TTC1_CLK2_PERIPHERAL_FREQMHZ": [ { "value": "133.333333", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_PCAP_PERIPHERAL_FREQMHZ": [ { "value": "200", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_TPIU_PERIPHERAL_FREQMHZ": [ { "value": "200", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_FPGA0_PERIPHERAL_FREQMHZ": [ { "value": "25", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_FPGA1_PERIPHERAL_FREQMHZ": [ { "value": "50", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_FPGA2_PERIPHERAL_FREQMHZ": [ { "value": "100", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_FPGA3_PERIPHERAL_FREQMHZ": [ { "value": "200", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_APU_PERIPHERAL_FREQMHZ": [ { "value": "666.666687", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_UIPARAM_ACT_DDR_FREQ_MHZ": [ { "value": "533.333374", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_DCI_PERIPHERAL_FREQMHZ": [ { "value": "10.158730", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_QSPI_PERIPHERAL_FREQMHZ": [ { "value": "142.857132", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_SMC_PERIPHERAL_FREQMHZ": [ { "value": "10.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_ENET0_PERIPHERAL_FREQMHZ": [ { "value": "125.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_ENET1_PERIPHERAL_FREQMHZ": [ { "value": "10.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_USB0_PERIPHERAL_FREQMHZ": [ { "value": "60", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_USB1_PERIPHERAL_FREQMHZ": [ { "value": "60", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_SDIO_PERIPHERAL_FREQMHZ": [ { "value": "100.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_UART_PERIPHERAL_FREQMHZ": [ { "value": "100.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_SPI_PERIPHERAL_FREQMHZ": [ { "value": "10.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_CAN_PERIPHERAL_FREQMHZ": [ { "value": "10.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_CAN0_PERIPHERAL_FREQMHZ": [ { "value": "23.8095", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_CAN1_PERIPHERAL_FREQMHZ": [ { "value": "23.8095", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_I2C_PERIPHERAL_FREQMHZ": [ { "value": "50", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_WDT_PERIPHERAL_FREQMHZ": [ { "value": "111.111115", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_TTC_PERIPHERAL_FREQMHZ": [ { "value": "50", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_PCAP_PERIPHERAL_FREQMHZ": [ { "value": "200.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_TPIU_PERIPHERAL_FREQMHZ": [ { "value": "200.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_FPGA0_PERIPHERAL_FREQMHZ": [ { "value": "25.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_FPGA1_PERIPHERAL_FREQMHZ": [ { "value": "50.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_FPGA2_PERIPHERAL_FREQMHZ": [ { "value": "100.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_FPGA3_PERIPHERAL_FREQMHZ": [ { "value": "200.000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_TTC0_CLK0_PERIPHERAL_FREQMHZ": [ { "value": "111.111115", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_TTC0_CLK1_PERIPHERAL_FREQMHZ": [ { "value": "111.111115", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_TTC0_CLK2_PERIPHERAL_FREQMHZ": [ { "value": "111.111115", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_TTC1_CLK0_PERIPHERAL_FREQMHZ": [ { "value": "111.111115", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_TTC1_CLK1_PERIPHERAL_FREQMHZ": [ { "value": "111.111115", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_ACT_TTC1_CLK2_PERIPHERAL_FREQMHZ": [ { "value": "111.111115", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_CLK0_FREQ": [ { "value": "25000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_CLK1_FREQ": [ { "value": "50000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_CLK2_FREQ": [ { "value": "100000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_CLK3_FREQ": [ { "value": "200000000", "value_src": "user", "resolve_type": "user", "format": "float", "usage": "all" } ],
        "PCW_OVERRIDE_BASIC_CLOCK": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_CPU_PERIPHERAL_DIVISOR0": [ { "value": "2", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_PERIPHERAL_DIVISOR0": [ { "value": "2", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SMC_PERIPHERAL_DIVISOR0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_QSPI_PERIPHERAL_DIVISOR0": [ { "value": "7", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SDIO_PERIPHERAL_DIVISOR0": [ { "value": "10", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_UART_PERIPHERAL_DIVISOR0": [ { "value": "10", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI_PERIPHERAL_DIVISOR0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_CAN_PERIPHERAL_DIVISOR0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_CAN_PERIPHERAL_DIVISOR1": [ { "value": "1", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FCLK0_PERIPHERAL_DIVISOR0": [ { "value": "8", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FCLK1_PERIPHERAL_DIVISOR0": [ { "value": "5", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FCLK2_PERIPHERAL_DIVISOR0": [ { "value": "5", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FCLK3_PERIPHERAL_DIVISOR0": [ { "value": "5", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FCLK0_PERIPHERAL_DIVISOR1": [ { "value": "5", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FCLK1_PERIPHERAL_DIVISOR1": [ { "value": "4", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FCLK2_PERIPHERAL_DIVISOR1": [ { "value": "2", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FCLK3_PERIPHERAL_DIVISOR1": [ { "value": "1", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_ENET0_PERIPHERAL_DIVISOR0": [ { "value": "8", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_ENET1_PERIPHERAL_DIVISOR0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_ENET0_PERIPHERAL_DIVISOR1": [ { "value": "1", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_ENET1_PERIPHERAL_DIVISOR1": [ { "value": "1", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TPIU_PERIPHERAL_DIVISOR0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DCI_PERIPHERAL_DIVISOR0": [ { "value": "15", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DCI_PERIPHERAL_DIVISOR1": [ { "value": "7", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_PCAP_PERIPHERAL_DIVISOR0": [ { "value": "5", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TTC0_CLK0_PERIPHERAL_DIVISOR0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC0_CLK1_PERIPHERAL_DIVISOR0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC0_CLK2_PERIPHERAL_DIVISOR0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC1_CLK0_PERIPHERAL_DIVISOR0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC1_CLK1_PERIPHERAL_DIVISOR0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC1_CLK2_PERIPHERAL_DIVISOR0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_WDT_PERIPHERAL_DIVISOR0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_ARMPLL_CTRL_FBDIV": [ { "value": "40", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_IOPLL_CTRL_FBDIV": [ { "value": "30", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDRPLL_CTRL_FBDIV": [ { "value": "32", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_CPU_CPU_PLL_FREQMHZ": [ { "value": "1333.333", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_IO_IO_PLL_FREQMHZ": [ { "value": "1000.000", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_DDR_PLL_FREQMHZ": [ { "value": "1066.667", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SMC_PERIPHERAL_VALID": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_SDIO_PERIPHERAL_VALID": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_SPI_PERIPHERAL_VALID": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_CAN_PERIPHERAL_VALID": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_UART_PERIPHERAL_VALID": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_CAN0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_CAN1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_ENET0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_ENET1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_PTP_ENET0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_PTP_ENET1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_GPIO": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_I2C0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_I2C1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_PJTAG": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_SDIO0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_CD_SDIO0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_WP_SDIO0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_SDIO1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_CD_SDIO1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_WP_SDIO1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_SPI0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_SPI1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_UART0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_UART1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_MODEM_UART0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_MODEM_UART1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_TTC0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_TTC1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_WDT": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_TRACE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_AXI_NONSECURE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_M_AXI_GP0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_M_AXI_GP1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_S_AXI_GP0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_S_AXI_GP1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_S_AXI_ACP": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_S_AXI_HP0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_S_AXI_HP1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_S_AXI_HP2": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_S_AXI_HP3": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_M_AXI_GP0_FREQMHZ": [ { "value": "100", "value_src": "propagated", "value_permission": "bd", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_M_AXI_GP1_FREQMHZ": [ { "value": "10", "value_permission": "bd", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_GP0_FREQMHZ": [ { "value": "10", "value_permission": "bd", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_GP1_FREQMHZ": [ { "value": "10", "value_permission": "bd", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_ACP_FREQMHZ": [ { "value": "10", "value_permission": "bd", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_HP0_FREQMHZ": [ { "value": "10", "value_permission": "bd", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_HP1_FREQMHZ": [ { "value": "10", "value_permission": "bd", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_HP2_FREQMHZ": [ { "value": "10", "value_permission": "bd", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_HP3_FREQMHZ": [ { "value": "10", "value_permission": "bd", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_USE_DMA0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_DMA1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_DMA2": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_DMA3": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_TRACE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_TRACE_PIPELINE_WIDTH": [ { "value": "8", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_INCLUDE_TRACE_BUFFER": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_BUFFER_FIFO_SIZE": [ { "value": "128", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_USE_TRACE_DATA_EDGE_DETECTOR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_BUFFER_CLOCK_DELAY": [ { "value": "12", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_USE_CROSS_TRIGGER": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_FTM_CTI_IN0": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FTM_CTI_IN1": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FTM_CTI_IN2": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FTM_CTI_IN3": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FTM_CTI_OUT0": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FTM_CTI_OUT1": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FTM_CTI_OUT2": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_FTM_CTI_OUT3": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_USE_DEBUG": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_CR_FABRIC": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_AXI_FABRIC_IDLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_DDR_BYPASS": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_FABRIC_INTERRUPT": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_PROC_EVENT_BUS": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_EXPANDED_IOP": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_HIGH_OCM": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_PS_SLCR_REGISTERS": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_EXPANDED_PS_SLCR_REGISTERS": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_USE_CORESIGHT": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_EMIO_SRAM_INT": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_GPIO_EMIO_GPIO_WIDTH": [ { "value": "64", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_GP0_NUM_WRITE_THREADS": [ { "value": "4", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_GP0_NUM_READ_THREADS": [ { "value": "4", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_GP1_NUM_WRITE_THREADS": [ { "value": "4", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_GP1_NUM_READ_THREADS": [ { "value": "4", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_UART0_BAUD_RATE": [ { "value": "115200", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_UART1_BAUD_RATE": [ { "value": "115200", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_4K_TIMER": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_M_AXI_GP0_ID_WIDTH": [ { "value": "12", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_M_AXI_GP0_ENABLE_STATIC_REMAP": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_M_AXI_GP0_SUPPORT_NARROW_BURST": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_M_AXI_GP0_THREAD_ID_WIDTH": [ { "value": "12", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_M_AXI_GP1_ID_WIDTH": [ { "value": "12", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_M_AXI_GP1_ENABLE_STATIC_REMAP": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_M_AXI_GP1_SUPPORT_NARROW_BURST": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_M_AXI_GP1_THREAD_ID_WIDTH": [ { "value": "12", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_GP0_ID_WIDTH": [ { "value": "6", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_GP1_ID_WIDTH": [ { "value": "6", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_ACP_ID_WIDTH": [ { "value": "3", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_INCLUDE_ACP_TRANS_CHECK": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_USE_DEFAULT_ACP_USER_VAL": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_ACP_ARUSER_VAL": [ { "value": "31", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_ACP_AWUSER_VAL": [ { "value": "31", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_HP0_ID_WIDTH": [ { "value": "6", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_HP0_DATA_WIDTH": [ { "value": "64", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_HP1_ID_WIDTH": [ { "value": "6", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_HP1_DATA_WIDTH": [ { "value": "64", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_HP2_ID_WIDTH": [ { "value": "6", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_HP2_DATA_WIDTH": [ { "value": "64", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_HP3_ID_WIDTH": [ { "value": "6", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_S_AXI_HP3_DATA_WIDTH": [ { "value": "64", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_NUM_F2P_INTR_INPUTS": [ { "value": "1", "value_permission": "bd", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_DDR": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_SMC": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_QSPI": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_CAN0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_CAN1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_ENET0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_ENET1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_GPIO": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_I2C0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_I2C1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_PJTAG": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_SDIO0": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_SDIO1": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_SPI0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_SPI1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_UART0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_UART1": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_MODEM_UART0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_MODEM_UART1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_TTC0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_TTC1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_WDT": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_TRACE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_USB0": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_USB1": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_DQ_WIDTH": [ { "value": "32", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_DQS_WIDTH": [ { "value": "4", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_DM_WIDTH": [ { "value": "4", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_MIO_PRIMITIVE": [ { "value": "54", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_CLK0_PORT": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_CLK1_PORT": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_CLK2_PORT": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_CLK3_PORT": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_RST0_PORT": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_RST1_PORT": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_RST2_PORT": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_RST3_PORT": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_CLKTRIG0_PORT": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_CLKTRIG1_PORT": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_CLKTRIG2_PORT": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_EN_CLKTRIG3_PORT": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_P2F_DMAC_ABORT_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_DMAC0_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_DMAC1_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_DMAC2_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_DMAC3_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_DMAC4_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_DMAC5_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_DMAC6_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_DMAC7_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_SMC_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_QSPI_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_CTI_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_GPIO_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_USB0_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_ENET0_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_SDIO0_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_I2C0_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_SPI0_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_UART0_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_CAN0_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_USB1_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_ENET1_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_SDIO1_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_I2C1_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_SPI1_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_UART1_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_P2F_CAN1_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_IRQ_F2P_INTR": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_IRQ_F2P_MODE": [ { "value": "DIRECT", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_CORE0_FIQ_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_CORE0_IRQ_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_CORE1_FIQ_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_CORE1_IRQ_INTR": [ { "value": "0", "value_src": "user", "resolve_type": "user", "format": "long", "enabled": false, "usage": "all" } ],
        "PCW_VALUE_SILVERSION": [ { "value": "3", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_GP0_EN_MODIFIABLE_TXN": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_GP1_EN_MODIFIABLE_TXN": [ { "value": "1", "value_src": "user", "resolve_type": "user", "format": "long", "usage": "all" } ],
        "PCW_IMPORT_BOARD_PRESET": [ { "value": "None", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_PERIPHERAL_BOARD_PRESET": [ { "value": "None", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_PRESET_BANK0_VOLTAGE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_PRESET_BANK1_VOLTAGE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_ADV_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_MEMORY_TYPE": [ { "value": "DDR 3", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_ECC": [ { "value": "Disabled", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_BUS_WIDTH": [ { "value": "32 Bit", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_BL": [ { "value": "8", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_HIGH_TEMP": [ { "value": "Normal (0-85)", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_PARTNO": [ { "value": "MT41J256M16 RE-125", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_DRAM_WIDTH": [ { "value": "16 Bits", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_DEVICE_CAPACITY": [ { "value": "4096 MBits", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_SPEED_BIN": [ { "value": "DDR3_1066F", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_UIPARAM_DDR_TRAIN_WRITE_LEVEL": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_TRAIN_READ_GATE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_TRAIN_DATA_EYE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_CLOCK_STOP_EN": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_DDR_USE_INTERNAL_VREF": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_DDR_PRIORITY_WRITEPORT_0": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_PRIORITY_WRITEPORT_1": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_PRIORITY_WRITEPORT_2": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_PRIORITY_WRITEPORT_3": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_PRIORITY_READPORT_0": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_PRIORITY_READPORT_1": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_PRIORITY_READPORT_2": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_PRIORITY_READPORT_3": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_PORT0_HPR_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_PORT1_HPR_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_PORT2_HPR_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_PORT3_HPR_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_HPRLPR_QUEUE_PARTITION": [ { "value": "HPR(0)/LPR(32)", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DDR_LPR_TO_CRITICAL_PRIORITY_LEVEL": [ { "value": "2", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_DDR_HPR_TO_CRITICAL_PRIORITY_LEVEL": [ { "value": "15", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_DDR_WRITE_TO_CRITICAL_PRIORITY_LEVEL": [ { "value": "2", "value_src": "user", "resolve_type": "user", "format": "float", "enabled": false, "usage": "all" } ],
        "PCW_NAND_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NAND_NAND_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NAND_GRP_D8_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NAND_GRP_D8_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_NOR_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_GRP_A25_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_GRP_A25_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_GRP_CS0_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_GRP_CS0_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_GRP_SRAM_CS0_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_GRP_SRAM_CS0_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_GRP_CS1_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_GRP_CS1_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_GRP_SRAM_CS1_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_GRP_SRAM_CS1_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_GRP_SRAM_INT_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_NOR_GRP_SRAM_INT_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_QSPI_PERIPHERAL_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_QSPI_QSPI_IO": [ { "value": "MIO 1 .. 6", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_QSPI_GRP_SINGLE_SS_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_QSPI_GRP_SINGLE_SS_IO": [ { "value": "MIO 1 .. 6", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_QSPI_GRP_SS1_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_QSPI_GRP_SS1_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SINGLE_QSPI_DATA_MODE": [ { "value": "x4", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_DUAL_STACK_QSPI_DATA_MODE": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_DUAL_PARALLEL_QSPI_DATA_MODE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_QSPI_GRP_IO1_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_QSPI_GRP_IO1_IO": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_QSPI_GRP_FBCLK_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_QSPI_GRP_FBCLK_IO": [ { "value": "MIO 8", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_QSPI_INTERNAL_HIGHADDRESS": [ { "value": "0xFCFFFFFF", "value_src": "user", "resolve_type": "user", "format": "bitString", "usage": "all" } ],
        "PCW_ENET0_PERIPHERAL_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_ENET0_ENET0_IO": [ { "value": "MIO 16 .. 27", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_ENET0_GRP_MDIO_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_ENET0_GRP_MDIO_IO": [ { "value": "MIO 52 .. 53", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_ENET_RESET_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_ENET_RESET_SELECT": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_ENET0_RESET_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_ENET0_RESET_IO": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_ENET1_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_ENET1_ENET1_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_ENET1_GRP_MDIO_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_ENET1_GRP_MDIO_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_ENET1_RESET_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_ENET1_RESET_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SD0_PERIPHERAL_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD0_SD0_IO": [ { "value": "MIO 40 .. 45", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD0_GRP_CD_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD0_GRP_CD_IO": [ { "value": "MIO 47", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD0_GRP_WP_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD0_GRP_WP_IO": [ { "value": "MIO 46", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD0_GRP_POW_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD0_GRP_POW_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SD1_PERIPHERAL_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD1_SD1_IO": [ { "value": "MIO 10 .. 15", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD1_GRP_CD_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD1_GRP_CD_IO": [ { "value": "MIO 9", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD1_GRP_WP_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD1_GRP_WP_IO": [ { "value": "MIO 0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD1_GRP_POW_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SD1_GRP_POW_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_UART0_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UART0_UART0_IO": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_UART0_GRP_FULL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_UART0_GRP_FULL_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_UART1_PERIPHERAL_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UART1_UART1_IO": [ { "value": "MIO 48 .. 49", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UART1_GRP_FULL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UART1_GRP_FULL_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI0_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SPI0_SPI0_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI0_GRP_SS0_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI0_GRP_SS0_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI0_GRP_SS1_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI0_GRP_SS1_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI0_GRP_SS2_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI0_GRP_SS2_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI1_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SPI1_SPI1_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI1_GRP_SS0_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI1_GRP_SS0_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI1_GRP_SS1_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI1_GRP_SS1_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI1_GRP_SS2_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_SPI1_GRP_SS2_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_CAN0_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_CAN0_CAN0_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_CAN0_GRP_CLK_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_CAN0_GRP_CLK_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_CAN1_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_CAN1_CAN1_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_CAN1_GRP_CLK_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_CAN1_GRP_CLK_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TRACE_TRACE_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_GRP_2BIT_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_GRP_2BIT_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_GRP_4BIT_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_GRP_4BIT_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_GRP_8BIT_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_GRP_8BIT_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_GRP_16BIT_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_GRP_16BIT_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_GRP_32BIT_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_GRP_32BIT_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TRACE_INTERNAL_WIDTH": [ { "value": "2", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_WDT_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_WDT_WDT_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TTC0_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC0_TTC0_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_TTC1_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC1_TTC1_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_PJTAG_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_PJTAG_PJTAG_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_USB0_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_USB0_USB0_IO": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_USB_RESET_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_USB_RESET_SELECT": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_USB0_RESET_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_USB0_RESET_IO": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_USB1_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_USB1_USB1_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_USB1_RESET_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_USB1_RESET_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_I2C0_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_I2C0_I2C0_IO": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_I2C0_GRP_INT_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_I2C0_GRP_INT_IO": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_I2C0_RESET_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_I2C0_RESET_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_I2C1_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_I2C1_I2C1_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_I2C1_GRP_INT_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_I2C1_GRP_INT_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_I2C_RESET_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_I2C_RESET_SELECT": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_I2C1_RESET_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_I2C1_RESET_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_GPIO_PERIPHERAL_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_GPIO_MIO_GPIO_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_GPIO_MIO_GPIO_IO": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_GPIO_EMIO_GPIO_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_GPIO_EMIO_GPIO_IO": [ { "value": "<Select>", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_APU_CLK_RATIO_ENABLE": [ { "value": "6:2:1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_ENET0_PERIPHERAL_FREQMHZ": [ { "value": "1000 Mbps", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_ENET1_PERIPHERAL_FREQMHZ": [ { "value": "1000 Mbps", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_CPU_PERIPHERAL_CLKSRC": [ { "value": "ARM PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_DDR_PERIPHERAL_CLKSRC": [ { "value": "DDR PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SMC_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_QSPI_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SDIO_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_UART_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SPI_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_CAN_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_FCLK0_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_FCLK1_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_FCLK2_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_FCLK3_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_ENET0_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_ENET1_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_CAN0_PERIPHERAL_CLKSRC": [ { "value": "External", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_CAN1_PERIPHERAL_CLKSRC": [ { "value": "External", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TPIU_PERIPHERAL_CLKSRC": [ { "value": "External", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC0_CLK0_PERIPHERAL_CLKSRC": [ { "value": "CPU_1X", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC0_CLK1_PERIPHERAL_CLKSRC": [ { "value": "CPU_1X", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC0_CLK2_PERIPHERAL_CLKSRC": [ { "value": "CPU_1X", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC1_CLK0_PERIPHERAL_CLKSRC": [ { "value": "CPU_1X", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC1_CLK1_PERIPHERAL_CLKSRC": [ { "value": "CPU_1X", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_TTC1_CLK2_PERIPHERAL_CLKSRC": [ { "value": "CPU_1X", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_WDT_PERIPHERAL_CLKSRC": [ { "value": "CPU_1X", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_DCI_PERIPHERAL_CLKSRC": [ { "value": "DDR PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_PCAP_PERIPHERAL_CLKSRC": [ { "value": "IO PLL", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_USB_RESET_POLARITY": [ { "value": "Active Low", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_ENET_RESET_POLARITY": [ { "value": "Active Low", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_I2C_RESET_POLARITY": [ { "value": "Active Low", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_0_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_0_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_0_DIRECTION": [ { "value": "in", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_0_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_1_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_1_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_1_DIRECTION": [ { "value": "out", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_1_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_2_PULLUP": [ { "value": "disabled", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_2_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_2_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_2_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_3_PULLUP": [ { "value": "disabled", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_3_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_3_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_3_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_4_PULLUP": [ { "value": "disabled", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_4_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_4_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_4_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_5_PULLUP": [ { "value": "disabled", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_5_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_5_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_5_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_6_PULLUP": [ { "value": "disabled", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_6_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_6_DIRECTION": [ { "value": "out", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_6_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_7_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_7_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_7_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_7_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_8_PULLUP": [ { "value": "disabled", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_8_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_8_DIRECTION": [ { "value": "out", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_8_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_9_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_9_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_9_DIRECTION": [ { "value": "in", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_9_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_10_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_10_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_10_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_10_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_11_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_11_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_11_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_11_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_12_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_12_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_12_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_12_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_13_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_13_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_13_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_13_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_14_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_14_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_14_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_14_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_15_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_15_IOTYPE": [ { "value": "LVCMOS 3.3V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_15_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_15_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_16_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_16_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_16_DIRECTION": [ { "value": "out", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_16_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_17_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_17_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_17_DIRECTION": [ { "value": "out", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_17_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_18_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_18_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_18_DIRECTION": [ { "value": "out", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_18_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_19_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_19_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_19_DIRECTION": [ { "value": "out", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_19_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_20_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_20_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_20_DIRECTION": [ { "value": "out", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_20_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_21_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_21_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_21_DIRECTION": [ { "value": "out", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_21_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_22_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_22_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_22_DIRECTION": [ { "value": "in", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_22_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_23_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_23_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_23_DIRECTION": [ { "value": "in", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_23_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_24_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_24_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_24_DIRECTION": [ { "value": "in", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_24_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_25_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_25_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_25_DIRECTION": [ { "value": "in", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_25_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_26_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_26_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_26_DIRECTION": [ { "value": "in", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_26_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_27_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_27_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_27_DIRECTION": [ { "value": "in", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_27_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_28_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_28_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_28_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_28_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_29_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_29_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_29_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_29_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_30_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_30_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_30_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_30_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_31_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_31_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_31_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_31_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_32_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_32_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_32_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_32_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_33_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_33_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_33_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_33_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_34_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_34_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_34_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_34_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_35_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_35_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_35_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_35_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_36_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_36_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_36_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_36_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_37_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_37_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_37_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_37_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_38_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_38_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_38_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_38_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_39_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_39_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_39_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_39_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_40_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_40_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_40_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_40_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_41_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_41_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_41_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_41_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_42_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_42_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_42_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_42_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_43_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_43_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_43_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_43_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_44_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_44_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_44_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_44_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_45_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_45_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_45_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_45_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_46_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_46_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_46_DIRECTION": [ { "value": "in", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_46_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_47_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_47_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_47_DIRECTION": [ { "value": "in", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_47_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_48_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_48_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_48_DIRECTION": [ { "value": "out", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_48_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_49_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_49_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_49_DIRECTION": [ { "value": "in", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_49_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_50_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_50_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_50_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_50_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_51_PULLUP": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_51_IOTYPE": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_51_DIRECTION": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_51_SLEW": [ { "value": "<Select>", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_52_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_52_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_52_DIRECTION": [ { "value": "out", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_52_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_53_PULLUP": [ { "value": "enabled", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_53_IOTYPE": [ { "value": "LVCMOS 1.8V", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_53_DIRECTION": [ { "value": "inout", "value_src": "user", "resolve_type": "user", "enabled": false, "usage": "all" } ],
        "PCW_MIO_53_SLEW": [ { "value": "slow", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "preset": [ { "value": "None", "resolve_type": "user", "usage": "all" } ],
        "PCW_UIPARAM_GENERATE_SUMMARY": [ { "value": "NA", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_TREE_PERIPHERALS": [ { "value": "SD 1#Quad SPI Flash#Quad SPI Flash#Quad SPI Flash#Quad SPI Flash#Quad SPI Flash#Quad SPI Flash#unassigned#Quad SPI Flash#SD 1#SD 1#SD 1#SD 1#SD 1#SD 1#SD 1#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#SD 0#SD 0#SD 0#SD 0#SD 0#SD 0#SD 0#SD 0#UART 1#UART 1#unassigned#unassigned#Enet 0#Enet 0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_MIO_TREE_SIGNALS": [ { "value": "wp#qspi0_ss_b#qspi0_io[0]#qspi0_io[1]#qspi0_io[2]#qspi0_io[3]/HOLD_B#qspi0_sclk#unassigned#qspi_fbclk#cd#data[0]#cmd#clk#data[1]#data[2]#data[3]#tx_clk#txd[0]#txd[1]#txd[2]#txd[3]#tx_ctl#rx_clk#rxd[0]#rxd[1]#rxd[2]#rxd[3]#rx_ctl#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#unassigned#clk#cmd#data[0]#data[1]#data[2]#data[3]#wp#cd#tx#rx#unassigned#unassigned#mdc#mdio", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_PS7_SI_REV": [ { "value": "PRODUCTION", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_FPGA_FCLK0_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_FPGA_FCLK1_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_FPGA_FCLK2_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_FPGA_FCLK3_ENABLE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS0_T_TR": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS0_T_PC": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS0_T_WP": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS0_T_CEOE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS0_T_WC": [ { "value": "11", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS0_T_RC": [ { "value": "11", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS0_WE_TIME": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS1_T_TR": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS1_T_PC": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS1_T_WP": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS1_T_CEOE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS1_T_WC": [ { "value": "11", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS1_T_RC": [ { "value": "11", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_SRAM_CS1_WE_TIME": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS0_T_TR": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS0_T_PC": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS0_T_WP": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS0_T_CEOE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS0_T_WC": [ { "value": "11", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS0_T_RC": [ { "value": "11", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS0_WE_TIME": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS1_T_TR": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS1_T_PC": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS1_T_WP": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS1_T_CEOE": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS1_T_WC": [ { "value": "11", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS1_T_RC": [ { "value": "11", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NOR_CS1_WE_TIME": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NAND_CYCLES_T_RR": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NAND_CYCLES_T_AR": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NAND_CYCLES_T_CLR": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NAND_CYCLES_T_WP": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NAND_CYCLES_T_REA": [ { "value": "1", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NAND_CYCLES_T_WC": [ { "value": "11", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_NAND_CYCLES_T_RC": [ { "value": "11", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SMC_CYCLE_T0": [ { "value": "NA", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SMC_CYCLE_T1": [ { "value": "NA", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SMC_CYCLE_T2": [ { "value": "NA", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SMC_CYCLE_T3": [ { "value": "NA", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SMC_CYCLE_T4": [ { "value": "NA", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SMC_CYCLE_T5": [ { "value": "NA", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_SMC_CYCLE_T6": [ { "value": "NA", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_PACKAGE_NAME": [ { "value": "ffg676", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "PCW_PLL_BYPASSMODE_ENABLE": [ { "value": "0", "value_src": "user", "resolve_type": "user", "usage": "all" } ],
        "Component_Name": [ { "value": "NewExtInst_TOP_processing_system7_0_0", "resolve_type": "user", "usage": "all" } ]
      },
      "model_parameters": {
        "C_EN_EMIO_PJTAG": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_EN_EMIO_ENET0": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_EN_EMIO_ENET1": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_EN_EMIO_TRACE": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_INCLUDE_TRACE_BUFFER": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_TRACE_BUFFER_FIFO_SIZE": [ { "value": "128", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "USE_TRACE_DATA_EDGE_DETECTOR": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_TRACE_PIPELINE_WIDTH": [ { "value": "8", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_TRACE_BUFFER_CLOCK_DELAY": [ { "value": "12", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_EMIO_GPIO_WIDTH": [ { "value": "64", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_INCLUDE_ACP_TRANS_CHECK": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_USE_DEFAULT_ACP_USER_VAL": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_ACP_ARUSER_VAL": [ { "value": "31", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_ACP_AWUSER_VAL": [ { "value": "31", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_M_AXI_GP0_ID_WIDTH": [ { "value": "12", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_M_AXI_GP0_ENABLE_STATIC_REMAP": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_M_AXI_GP1_ID_WIDTH": [ { "value": "12", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_M_AXI_GP1_ENABLE_STATIC_REMAP": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_GP0_ID_WIDTH": [ { "value": "6", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_GP1_ID_WIDTH": [ { "value": "6", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_ACP_ID_WIDTH": [ { "value": "3", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_HP0_ID_WIDTH": [ { "value": "6", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_HP0_DATA_WIDTH": [ { "value": "64", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_HP1_ID_WIDTH": [ { "value": "6", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_HP1_DATA_WIDTH": [ { "value": "64", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_HP2_ID_WIDTH": [ { "value": "6", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_HP2_DATA_WIDTH": [ { "value": "64", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_HP3_ID_WIDTH": [ { "value": "6", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_S_AXI_HP3_DATA_WIDTH": [ { "value": "64", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_M_AXI_GP0_THREAD_ID_WIDTH": [ { "value": "12", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_M_AXI_GP1_THREAD_ID_WIDTH": [ { "value": "12", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_NUM_F2P_INTR_INPUTS": [ { "value": "1", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_IRQ_F2P_MODE": [ { "value": "DIRECT", "resolve_type": "dependent", "usage": "all" } ],
        "C_DQ_WIDTH": [ { "value": "32", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_DQS_WIDTH": [ { "value": "4", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_DM_WIDTH": [ { "value": "4", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_MIO_PRIMITIVE": [ { "value": "54", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_TRACE_INTERNAL_WIDTH": [ { "value": "2", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_USE_AXI_NONSECURE": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_USE_M_AXI_GP0": [ { "value": "1", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_USE_M_AXI_GP1": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_USE_S_AXI_GP0": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_USE_S_AXI_GP1": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_USE_S_AXI_HP0": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_USE_S_AXI_HP1": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_USE_S_AXI_HP2": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_USE_S_AXI_HP3": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_USE_S_AXI_ACP": [ { "value": "0", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_PS7_SI_REV": [ { "value": "PRODUCTION", "resolve_type": "dependent", "usage": "all" } ],
        "C_FCLK_CLK0_BUF": [ { "value": "TRUE", "resolve_type": "dependent", "usage": "all" } ],
        "C_FCLK_CLK1_BUF": [ { "value": "TRUE", "resolve_type": "dependent", "usage": "all" } ],
        "C_FCLK_CLK2_BUF": [ { "value": "TRUE", "resolve_type": "dependent", "usage": "all" } ],
        "C_FCLK_CLK3_BUF": [ { "value": "TRUE", "resolve_type": "dependent", "usage": "all" } ],
        "C_PACKAGE_NAME": [ { "value": "ffg676", "resolve_type": "dependent", "usage": "all" } ],
        "C_GP0_EN_MODIFIABLE_TXN": [ { "value": "1", "resolve_type": "dependent", "format": "long", "usage": "all" } ],
        "C_GP1_EN_MODIFIABLE_TXN": [ { "value": "1", "resolve_type": "dependent", "format": "long", "usage": "all" } ]
      },
      "project_parameters": {
        "ARCHITECTURE": [ { "value": "zynq" } ],
        "BASE_BOARD_PART": [ { "value": "" } ],
        "BOARD_CONNECTIONS": [ { "value": "" } ],
        "DEVICE": [ { "value": "xc7z035" } ],
        "PACKAGE": [ { "value": "ffg676" } ],
        "PREFHDL": [ { "value": "VERILOG" } ],
        "SILICON_REVISION": [ { "value": "" } ],
        "SIMULATOR_LANGUAGE": [ { "value": "MIXED" } ],
        "SPEEDGRADE": [ { "value": "-2" } ],
        "STATIC_POWER": [ { "value": "" } ],
        "TEMPERATURE_GRADE": [ { "value": "" } ],
        "USE_RDI_CUSTOMIZATION": [ { "value": "TRUE" } ],
        "USE_RDI_GENERATION": [ { "value": "TRUE" } ]
      },
      "runtime_parameters": {
        "IPCONTEXT": [ { "value": "IP_Integrator" } ],
        "IPREVISION": [ { "value": "6" } ],
        "MANAGED": [ { "value": "TRUE" } ],
        "OUTPUTDIR": [ { "value": "../../../../../../NewExtInst_Debug.gen/sources_1/bd/NewExtInst_TOP/ip/NewExtInst_TOP_processing_system7_0_0" } ],
        "SELECTEDSIMMODEL": [ { "value": "" } ],
        "SHAREDDIR": [ { "value": "../../ipshared" } ],
        "SWVERSION": [ { "value": "2023.2" } ],
        "SYNTHESISFLOW": [ { "value": "OUT_OF_CONTEXT" } ]
      }
    },
    "boundary": {
      "ports": {
        "M_AXI_GP0_ARVALID": [ { "direction": "out" } ],
        "M_AXI_GP0_AWVALID": [ { "direction": "out" } ],
        "M_AXI_GP0_BREADY": [ { "direction": "out" } ],
        "M_AXI_GP0_RREADY": [ { "direction": "out" } ],
        "M_AXI_GP0_WLAST": [ { "direction": "out" } ],
        "M_AXI_GP0_WVALID": [ { "direction": "out" } ],
        "M_AXI_GP0_ARID": [ { "direction": "out", "size_left": "11", "size_right": "0" } ],
        "M_AXI_GP0_AWID": [ { "direction": "out", "size_left": "11", "size_right": "0" } ],
        "M_AXI_GP0_WID": [ { "direction": "out", "size_left": "11", "size_right": "0" } ],
        "M_AXI_GP0_ARBURST": [ { "direction": "out", "size_left": "1", "size_right": "0" } ],
        "M_AXI_GP0_ARLOCK": [ { "direction": "out", "size_left": "1", "size_right": "0" } ],
        "M_AXI_GP0_ARSIZE": [ { "direction": "out", "size_left": "2", "size_right": "0" } ],
        "M_AXI_GP0_AWBURST": [ { "direction": "out", "size_left": "1", "size_right": "0" } ],
        "M_AXI_GP0_AWLOCK": [ { "direction": "out", "size_left": "1", "size_right": "0" } ],
        "M_AXI_GP0_AWSIZE": [ { "direction": "out", "size_left": "2", "size_right": "0" } ],
        "M_AXI_GP0_ARPROT": [ { "direction": "out", "size_left": "2", "size_right": "0" } ],
        "M_AXI_GP0_AWPROT": [ { "direction": "out", "size_left": "2", "size_right": "0" } ],
        "M_AXI_GP0_ARADDR": [ { "direction": "out", "size_left": "31", "size_right": "0" } ],
        "M_AXI_GP0_AWADDR": [ { "direction": "out", "size_left": "31", "size_right": "0" } ],
        "M_AXI_GP0_WDATA": [ { "direction": "out", "size_left": "31", "size_right": "0" } ],
        "M_AXI_GP0_ARCACHE": [ { "direction": "out", "size_left": "3", "size_right": "0" } ],
        "M_AXI_GP0_ARLEN": [ { "direction": "out", "size_left": "3", "size_right": "0" } ],
        "M_AXI_GP0_ARQOS": [ { "direction": "out", "size_left": "3", "size_right": "0" } ],
        "M_AXI_GP0_AWCACHE": [ { "direction": "out", "size_left": "3", "size_right": "0" } ],
        "M_AXI_GP0_AWLEN": [ { "direction": "out", "size_left": "3", "size_right": "0" } ],
        "M_AXI_GP0_AWQOS": [ { "direction": "out", "size_left": "3", "size_right": "0" } ],
        "M_AXI_GP0_WSTRB": [ { "direction": "out", "size_left": "3", "size_right": "0" } ],
        "M_AXI_GP0_ACLK": [ { "direction": "in", "driver_value": "0" } ],
        "M_AXI_GP0_ARREADY": [ { "direction": "in", "driver_value": "0" } ],
        "M_AXI_GP0_AWREADY": [ { "direction": "in", "driver_value": "0" } ],
        "M_AXI_GP0_BVALID": [ { "direction": "in", "driver_value": "0" } ],
        "M_AXI_GP0_RLAST": [ { "direction": "in", "driver_value": "0" } ],
        "M_AXI_GP0_RVALID": [ { "direction": "in", "driver_value": "0" } ],
        "M_AXI_GP0_WREADY": [ { "direction": "in", "driver_value": "0" } ],
        "M_AXI_GP0_BID": [ { "direction": "in", "size_left": "11", "size_right": "0", "driver_value": "0" } ],
        "M_AXI_GP0_RID": [ { "direction": "in", "size_left": "11", "size_right": "0", "driver_value": "0" } ],
        "M_AXI_GP0_BRESP": [ { "direction": "in", "size_left": "1", "size_right": "0", "driver_value": "0" } ],
        "M_AXI_GP0_RRESP": [ { "direction": "in", "size_left": "1", "size_right": "0", "driver_value": "0" } ],
        "M_AXI_GP0_RDATA": [ { "direction": "in", "size_left": "31", "size_right": "0", "driver_value": "0" } ],
        "FCLK_CLK0": [ { "direction": "out" } ],
        "FCLK_CLK1": [ { "direction": "out" } ],
        "FCLK_CLK2": [ { "direction": "out" } ],
        "FCLK_CLK3": [ { "direction": "out" } ],
        "FCLK_RESET0_N": [ { "direction": "out" } ],
        "MIO": [ { "direction": "inout", "size_left": "53", "size_right": "0" } ],
        "DDR_CAS_n": [ { "direction": "inout" } ],
        "DDR_CKE": [ { "direction": "inout" } ],
        "DDR_Clk_n": [ { "direction": "inout" } ],
        "DDR_Clk": [ { "direction": "inout" } ],
        "DDR_CS_n": [ { "direction": "inout" } ],
        "DDR_DRSTB": [ { "direction": "inout" } ],
        "DDR_ODT": [ { "direction": "inout" } ],
        "DDR_RAS_n": [ { "direction": "inout" } ],
        "DDR_WEB": [ { "direction": "inout" } ],
        "DDR_BankAddr": [ { "direction": "inout", "size_left": "2", "size_right": "0" } ],
        "DDR_Addr": [ { "direction": "inout", "size_left": "14", "size_right": "0" } ],
        "DDR_VRN": [ { "direction": "inout" } ],
        "DDR_VRP": [ { "direction": "inout" } ],
        "DDR_DM": [ { "direction": "inout", "size_left": "3", "size_right": "0" } ],
        "DDR_DQ": [ { "direction": "inout", "size_left": "31", "size_right": "0" } ],
        "DDR_DQS_n": [ { "direction": "inout", "size_left": "3", "size_right": "0" } ],
        "DDR_DQS": [ { "direction": "inout", "size_left": "3", "size_right": "0" } ],
        "PS_SRSTB": [ { "direction": "inout" } ],
        "PS_CLK": [ { "direction": "inout" } ],
        "PS_PORB": [ { "direction": "inout" } ]
      },
      "interfaces": {
        "DDR": {
          "vlnv": "xilinx.com:interface:ddrx:1.0",
          "abstraction_type": "xilinx.com:interface:ddrx_rtl:1.0",
          "mode": "master",
          "parameters": {
            "CAN_DEBUG": [ { "value": "false", "value_permission": "bd", "resolve_type": "generated", "format": "bool", "is_static_object": false } ],
            "TIMEPERIOD_PS": [ { "value": "1250", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "MEMORY_TYPE": [ { "value": "COMPONENTS", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "MEMORY_PART": [ { "value": "", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "DATA_WIDTH": [ { "value": "8", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "CS_ENABLED": [ { "value": "true", "value_permission": "bd", "resolve_type": "generated", "format": "bool", "is_static_object": false } ],
            "DATA_MASK_ENABLED": [ { "value": "true", "value_permission": "bd", "resolve_type": "generated", "format": "bool", "is_static_object": false } ],
            "SLOT": [ { "value": "Single", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "CUSTOM_PARTS": [ { "value": "", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "MEM_ADDR_MAP": [ { "value": "ROW_COLUMN_BANK", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "BURST_LENGTH": [ { "value": "8", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "AXI_ARBITRATION_SCHEME": [ { "value": "TDM", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "CAS_LATENCY": [ { "value": "11", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "CAS_WRITE_LATENCY": [ { "value": "11", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ]
          },
          "port_maps": {
            "CAS_N": [ { "physical_name": "DDR_CAS_n" } ],
            "CKE": [ { "physical_name": "DDR_CKE" } ],
            "CK_N": [ { "physical_name": "DDR_Clk_n" } ],
            "CK_P": [ { "physical_name": "DDR_Clk" } ],
            "CS_N": [ { "physical_name": "DDR_CS_n" } ],
            "RESET_N": [ { "physical_name": "DDR_DRSTB" } ],
            "ODT": [ { "physical_name": "DDR_ODT" } ],
            "RAS_N": [ { "physical_name": "DDR_RAS_n" } ],
            "WE_N": [ { "physical_name": "DDR_WEB" } ],
            "BA": [ { "physical_name": "DDR_BankAddr" } ],
            "ADDR": [ { "physical_name": "DDR_Addr" } ],
            "DM": [ { "physical_name": "DDR_DM" } ],
            "DQ": [ { "physical_name": "DDR_DQ" } ],
            "DQS_N": [ { "physical_name": "DDR_DQS_n" } ],
            "DQS_P": [ { "physical_name": "DDR_DQS" } ]
          }
        },
        "FIXED_IO": {
          "vlnv": "xilinx.com:display_processing_system7:fixedio:1.0",
          "abstraction_type": "xilinx.com:display_processing_system7:fixedio_rtl:1.0",
          "mode": "master",
          "parameters": {
            "CAN_DEBUG": [ { "value": "false", "value_permission": "bd", "resolve_type": "generated", "format": "bool", "is_static_object": false } ]
          },
          "port_maps": {
            "MIO": [ { "physical_name": "MIO" } ],
            "DDR_VRN": [ { "physical_name": "DDR_VRN" } ],
            "DDR_VRP": [ { "physical_name": "DDR_VRP" } ],
            "PS_SRSTB": [ { "physical_name": "PS_SRSTB" } ],
            "PS_CLK": [ { "physical_name": "PS_CLK" } ],
            "PS_PORB": [ { "physical_name": "PS_PORB" } ]
          }
        },
        "M_AXI_GP0": {
          "vlnv": "xilinx.com:interface:aximm:1.0",
          "abstraction_type": "xilinx.com:interface:aximm_rtl:1.0",
          "mode": "master",
          "address_space_ref": "Data",
          "parameters": {
            "SUPPORTS_NARROW_BURST": [ { "value": "0", "value_src": "user", "value_permission": "bd", "resolve_type": "generated", "format": "long", "usage": "all" } ],
            "NUM_WRITE_OUTSTANDING": [ { "value": "8", "value_src": "constant", "value_permission": "bd", "usage": "all" } ],
            "NUM_READ_OUTSTANDING": [ { "value": "8", "value_src": "constant", "value_permission": "bd", "usage": "all" } ],
            "DATA_WIDTH": [ { "value": "32", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "PROTOCOL": [ { "value": "AXI3", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "FREQ_HZ": [ { "value": "100000000", "value_src": "ip_propagated", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "ID_WIDTH": [ { "value": "12", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "ADDR_WIDTH": [ { "value": "32", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "AWUSER_WIDTH": [ { "value": "0", "value_src": "constant", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "ARUSER_WIDTH": [ { "value": "0", "value_src": "constant", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "WUSER_WIDTH": [ { "value": "0", "value_src": "constant", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "RUSER_WIDTH": [ { "value": "0", "value_src": "constant", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "BUSER_WIDTH": [ { "value": "0", "value_src": "constant", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "READ_WRITE_MODE": [ { "value": "READ_WRITE", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "HAS_BURST": [ { "value": "1", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "HAS_LOCK": [ { "value": "1", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "HAS_PROT": [ { "value": "1", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "HAS_CACHE": [ { "value": "1", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "HAS_QOS": [ { "value": "1", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "HAS_REGION": [ { "value": "0", "value_src": "constant", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "HAS_WSTRB": [ { "value": "1", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "HAS_BRESP": [ { "value": "1", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "HAS_RRESP": [ { "value": "1", "value_src": "auto", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "MAX_BURST_LENGTH": [ { "value": "16", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "PHASE": [ { "value": "0.0", "value_src": "ip_propagated", "value_permission": "bd", "resolve_type": "generated", "format": "float", "is_static_object": false } ],
            "CLK_DOMAIN": [ { "value": "/clk_wiz_0_clk_out1", "value_src": "ip_propagated", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "NUM_READ_THREADS": [ { "value": "4", "value_src": "constant", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "NUM_WRITE_THREADS": [ { "value": "4", "value_src": "constant", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "RUSER_BITS_PER_BYTE": [ { "value": "0", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "WUSER_BITS_PER_BYTE": [ { "value": "0", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "INSERT_VIP": [ { "value": "0", "resolve_type": "user", "format": "long", "usage": "simulation.rtl", "is_static_object": false } ]
          },
          "port_maps": {
            "ARVALID": [ { "physical_name": "M_AXI_GP0_ARVALID" } ],
            "AWVALID": [ { "physical_name": "M_AXI_GP0_AWVALID" } ],
            "BREADY": [ { "physical_name": "M_AXI_GP0_BREADY" } ],
            "RREADY": [ { "physical_name": "M_AXI_GP0_RREADY" } ],
            "WLAST": [ { "physical_name": "M_AXI_GP0_WLAST" } ],
            "WVALID": [ { "physical_name": "M_AXI_GP0_WVALID" } ],
            "ARID": [ { "physical_name": "M_AXI_GP0_ARID" } ],
            "AWID": [ { "physical_name": "M_AXI_GP0_AWID" } ],
            "WID": [ { "physical_name": "M_AXI_GP0_WID" } ],
            "ARBURST": [ { "physical_name": "M_AXI_GP0_ARBURST" } ],
            "ARLOCK": [ { "physical_name": "M_AXI_GP0_ARLOCK" } ],
            "ARSIZE": [ { "physical_name": "M_AXI_GP0_ARSIZE" } ],
            "AWBURST": [ { "physical_name": "M_AXI_GP0_AWBURST" } ],
            "AWLOCK": [ { "physical_name": "M_AXI_GP0_AWLOCK" } ],
            "AWSIZE": [ { "physical_name": "M_AXI_GP0_AWSIZE" } ],
            "ARPROT": [ { "physical_name": "M_AXI_GP0_ARPROT" } ],
            "AWPROT": [ { "physical_name": "M_AXI_GP0_AWPROT" } ],
            "ARADDR": [ { "physical_name": "M_AXI_GP0_ARADDR" } ],
            "AWADDR": [ { "physical_name": "M_AXI_GP0_AWADDR" } ],
            "WDATA": [ { "physical_name": "M_AXI_GP0_WDATA" } ],
            "ARCACHE": [ { "physical_name": "M_AXI_GP0_ARCACHE" } ],
            "ARLEN": [ { "physical_name": "M_AXI_GP0_ARLEN" } ],
            "ARQOS": [ { "physical_name": "M_AXI_GP0_ARQOS" } ],
            "AWCACHE": [ { "physical_name": "M_AXI_GP0_AWCACHE" } ],
            "AWLEN": [ { "physical_name": "M_AXI_GP0_AWLEN" } ],
            "AWQOS": [ { "physical_name": "M_AXI_GP0_AWQOS" } ],
            "WSTRB": [ { "physical_name": "M_AXI_GP0_WSTRB" } ],
            "ARREADY": [ { "physical_name": "M_AXI_GP0_ARREADY" } ],
            "AWREADY": [ { "physical_name": "M_AXI_GP0_AWREADY" } ],
            "BVALID": [ { "physical_name": "M_AXI_GP0_BVALID" } ],
            "RLAST": [ { "physical_name": "M_AXI_GP0_RLAST" } ],
            "RVALID": [ { "physical_name": "M_AXI_GP0_RVALID" } ],
            "WREADY": [ { "physical_name": "M_AXI_GP0_WREADY" } ],
            "BID": [ { "physical_name": "M_AXI_GP0_BID" } ],
            "RID": [ { "physical_name": "M_AXI_GP0_RID" } ],
            "BRESP": [ { "physical_name": "M_AXI_GP0_BRESP" } ],
            "RRESP": [ { "physical_name": "M_AXI_GP0_RRESP" } ],
            "RDATA": [ { "physical_name": "M_AXI_GP0_RDATA" } ]
          }
        },
        "FCLK_CLK0": {
          "vlnv": "xilinx.com:signal:clock:1.0",
          "abstraction_type": "xilinx.com:signal:clock_rtl:1.0",
          "mode": "master",
          "parameters": {
            "FREQ_HZ": [ { "value": "25000000", "value_src": "user", "value_permission": "bd", "resolve_type": "generated", "format": "float", "usage": "all" } ],
            "PHASE": [ { "value": "0.000", "value_permission": "bd", "resolve_type": "generated", "format": "float", "is_static_object": false } ],
            "CLK_DOMAIN": [ { "value": "NewExtInst_TOP_processing_system7_0_0_FCLK_CLK0", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "ASSOCIATED_BUSIF": [ { "value": "", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "ASSOCIATED_RESET": [ { "value": "", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "INSERT_VIP": [ { "value": "0", "resolve_type": "user", "format": "long", "usage": "simulation.rtl", "is_static_object": false } ]
          },
          "port_maps": {
            "CLK": [ { "physical_name": "FCLK_CLK0" } ]
          }
        },
        "FCLK_CLK1": {
          "vlnv": "xilinx.com:signal:clock:1.0",
          "abstraction_type": "xilinx.com:signal:clock_rtl:1.0",
          "mode": "master",
          "parameters": {
            "FREQ_HZ": [ { "value": "50000000", "value_src": "user", "value_permission": "bd", "resolve_type": "generated", "format": "float", "usage": "all" } ],
            "PHASE": [ { "value": "0.000", "value_permission": "bd", "resolve_type": "generated", "format": "float", "is_static_object": false } ],
            "CLK_DOMAIN": [ { "value": "NewExtInst_TOP_processing_system7_0_0_FCLK_CLK1", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "ASSOCIATED_BUSIF": [ { "value": "", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "ASSOCIATED_RESET": [ { "value": "", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "INSERT_VIP": [ { "value": "0", "resolve_type": "user", "format": "long", "usage": "simulation.rtl", "is_static_object": false } ]
          },
          "port_maps": {
            "CLK": [ { "physical_name": "FCLK_CLK1" } ]
          }
        },
        "FCLK_CLK2": {
          "vlnv": "xilinx.com:signal:clock:1.0",
          "abstraction_type": "xilinx.com:signal:clock_rtl:1.0",
          "mode": "master",
          "parameters": {
            "FREQ_HZ": [ { "value": "100000000", "value_src": "user", "value_permission": "bd", "resolve_type": "generated", "format": "float", "usage": "all" } ],
            "PHASE": [ { "value": "0.000", "value_permission": "bd", "resolve_type": "generated", "format": "float", "is_static_object": false } ],
            "CLK_DOMAIN": [ { "value": "NewExtInst_TOP_processing_system7_0_0_FCLK_CLK2", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "ASSOCIATED_BUSIF": [ { "value": "", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "ASSOCIATED_RESET": [ { "value": "", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "INSERT_VIP": [ { "value": "0", "resolve_type": "user", "format": "long", "usage": "simulation.rtl", "is_static_object": false } ]
          },
          "port_maps": {
            "CLK": [ { "physical_name": "FCLK_CLK2" } ]
          }
        },
        "FCLK_CLK3": {
          "vlnv": "xilinx.com:signal:clock:1.0",
          "abstraction_type": "xilinx.com:signal:clock_rtl:1.0",
          "mode": "master",
          "parameters": {
            "FREQ_HZ": [ { "value": "200000000", "value_src": "user", "value_permission": "bd", "resolve_type": "generated", "format": "float", "usage": "all" } ],
            "PHASE": [ { "value": "0.000", "value_permission": "bd", "resolve_type": "generated", "format": "float", "is_static_object": false } ],
            "CLK_DOMAIN": [ { "value": "NewExtInst_TOP_processing_system7_0_0_FCLK_CLK3", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "ASSOCIATED_BUSIF": [ { "value": "", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "ASSOCIATED_RESET": [ { "value": "", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "INSERT_VIP": [ { "value": "0", "resolve_type": "user", "format": "long", "usage": "simulation.rtl", "is_static_object": false } ]
          },
          "port_maps": {
            "CLK": [ { "physical_name": "FCLK_CLK3" } ]
          }
        },
        "FCLK_RESET0_N": {
          "vlnv": "xilinx.com:signal:reset:1.0",
          "abstraction_type": "xilinx.com:signal:reset_rtl:1.0",
          "mode": "master",
          "parameters": {
            "POLARITY": [ { "value": "ACTIVE_LOW", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "INSERT_VIP": [ { "value": "0", "resolve_type": "user", "format": "long", "usage": "simulation.rtl", "is_static_object": false } ]
          },
          "port_maps": {
            "RST": [ { "physical_name": "FCLK_RESET0_N" } ]
          }
        },
        "M_AXI_GP0_ACLK": {
          "vlnv": "xilinx.com:signal:clock:1.0",
          "abstraction_type": "xilinx.com:signal:clock_rtl:1.0",
          "mode": "slave",
          "parameters": {
            "ASSOCIATED_BUSIF": [ { "value": "M_AXI_GP0", "value_src": "constant", "value_permission": "bd", "usage": "all" } ],
            "FREQ_HZ": [ { "value": "100000000", "value_src": "ip_propagated", "value_permission": "bd", "resolve_type": "generated", "format": "long", "is_static_object": false } ],
            "PHASE": [ { "value": "0.0", "value_src": "ip_propagated", "value_permission": "bd", "resolve_type": "generated", "format": "float", "is_static_object": false } ],
            "CLK_DOMAIN": [ { "value": "/clk_wiz_0_clk_out1", "value_src": "ip_propagated", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "ASSOCIATED_RESET": [ { "value": "", "value_permission": "bd", "resolve_type": "generated", "is_static_object": false } ],
            "INSERT_VIP": [ { "value": "0", "resolve_type": "user", "format": "long", "usage": "simulation.rtl", "is_static_object": false } ]
          },
          "port_maps": {
            "CLK": [ { "physical_name": "M_AXI_GP0_ACLK" } ]
          }
        }
      },
      "address_spaces": {
        "Data": {
          "range": "4G",
          "display_name": "Data",
          "width": "32",
          "apertures": {
            "segment1": [ { "offset": "0x00000000", "range": "0x00040000", "display_name": "segment1" } ],
            "segment2": [ { "offset": "0x00040000", "range": "0x00040000", "display_name": "segment2" } ],
            "segment3": [ { "offset": "0x00080000", "range": "0x00080000", "display_name": "segment3" } ],
            "segment4": [ { "offset": "0x00100000", "range": "0x3ff00000", "display_name": "segment4" } ],
            "M_AXI_GP0": [ { "offset": "0x40000000", "range": "0x40000000", "display_name": "M_AXI_GP0" } ],
            "M_AXI_GP1": [ { "offset": "0x80000000", "range": "0x40000000", "display_name": "M_AXI_GP1" } ],
            "IO_Peripheral_Registers": [ { "offset": "0xe0000000", "range": "0x00300000", "display_name": "IO Peripheral Registers" } ],
            "SMC_Memories": [ { "offset": "0xe1000000", "range": "0x05000000", "display_name": "SMC Memories" } ],
            "SLCR_Registers": [ { "offset": "0xf8000000", "range": "0x00000c00", "display_name": "SLCR Registers" } ],
            "PS_System_Registers": [ { "offset": "0xf8001000", "range": "0x0080f000", "display_name": "PS System Registers" } ],
            "CPU_Private_Registers": [ { "offset": "0xf8900000", "range": "0x00603000", "display_name": "CPU Private Registers" } ],
            "segment5": [ { "offset": "0xfc000000", "range": "0x02000000", "display_name": "segment5" } ],
            "segment6": [ { "offset": "0xfffc0000", "range": "0x00040000", "display_name": "segment6" } ]
          }
        }
      }
    },
    "contents": {
      "cpus": {
        "CPU0_A9": {
          "address_space_refs": "Data",
          "parameters": {
            "is_visible": [ { "value": "FALSE" } ],
            "processor_type": [ { "value": "ARM" } ]
          }
        },
        "CPU1_A9": {
          "address_space_refs": "Data",
          "parameters": {
            "is_visible": [ { "value": "FALSE" } ],
            "processor_type": [ { "value": "ARM" } ]
          }
        }
      }
    }
  }
}